{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":4,"rows_kept":6,"merged":[[0,0,0,3],[5,0,5,3]],"flags":["formulas_cached_only"]}
["附件一：调研产品清单及需求"]
["序号","耗材名称","用途及参数需求","其他需求"]
[1,"血液净化装置的体外循环管路","1、可应用于血液透析(HD)、血液滤过(HF)和血液透析滤过(HDF)等不同血液净化治疗模式\n2、符合 SOP 使用指引，具备密闭式预充和回血\n3、管路各项监测接口、液体接口完备，可确保血液在治疗过程中顺畅流动和交换，并保证血流动力学稳定性\n4、管路材具有良好的生物相容性，可有效避免过敏、炎症等不良反应\n5、具备密闭式预充和回血通路，预充输液管可分离可调节速度\n6、废液(积液)袋有Y型接头，带止血夹，可循管","一、如有必须配合使用的配套设备、耗材等，需一起报名\n二、具备医疗器械注册证\n三、广州集采中选产品，已纳入《广州市社会医疗保险及生育保险医用耗材目录》"]
[2,"腔道用耦合剂套装","1、无菌型耦合剂需满足无菌要求，消毒型耦合剂应能杀灭和抑制探头与人体接触引起的病原性革兰氏菌、粪大肠菌落、绿脓杆菌、真菌等，有效防止交叉感染。\n2、隔离膜具备一定抗拉强度、柔韧性和耐穿刺性。\n3、采用卡套一体化设计，套内预充具有杀菌性能耦合剂的无菌耦合剂，使用安全方便预防院内交叉感染。\n4、符合国家药监局对腔道用耦合剂 Y0299-2022 最新强制标准要求。","一、如有必须配合使用的配套设备、耗材等，需一起报名\n二、具备医疗器械注册证\n三、已纳入《广州市社会医疗保险及生育保险医用耗材目录》"]
[]
["声明：以上所述的初步配置及参数需求等要求无指向性、倾向性和排他性，因市场了解的局限性，可能存在不足，仅作为本次市场调研参考用。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}